[4] CORROSION PROTECTION - - WAX INJECTION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

WAX INJECTION LOCATIONS
[EXCEPT FOR HONG KONG SPEC] In order to provide greater corrosion resistance, wax injection has been performed for the lower areas of the vehicle, such as the frame, the side sill, and other panels which are a hollow-construction. If any of these panels are replaced, wax injection must be performed for the new parts. Recommended wax: Tectyl 506, 506T or ML Waxoyl Dinitrol 3122 or 3654-1 Mercasol 831-ML Terotex HV200PLUS or HV300
NOTES REGARDING WAX INJECTION WORK Be careful that the wax does not get onto other parts. Especially if wax is to be injected into the lower part of the centre pillar and into the side sill, first remove the seat belt retractor and the door switch. For wax injection locations which have a rubber plug, do not forget to reinstall the rubber plug after the wax injection is completed. NOTE: For the numbers shown in the figure, refer to detailed illustrations with the same numbers on later pages.

[4] CORROSION PROTECTION - - WAX INJECTION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation