[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - ON-VEHICLE SERVICE - PROCEDURE FOR INPUT OF SECURITY CODE FOR ANTI-THEFT SYSTEM <Vehicles for Australia and New zealand> | PRINT PAGE / INDEX / PRIOR / NEXT

| ON-VEHICLE SERVICE

| PROCEDURE FOR INPUT OF SECURITY CODE FOR ANTI-THEFT SYSTEM <Vehicles for Australia and New zealand> The radio and CD player do not work under the following conditions:
| If the ignition key is removed, the security indicator of this radio and CD player flickers to prevent theft from happening. Power supply to the radio and CD player has been suspended for more than an hour continuously by removing the cable from the battery terminal or disconnecting the harness connectors. The power supply to the radio and CD player has been suspended for more than an hour due to a blown fuse or discharged battery. If the radio and CD player does not work for these conditions, enter the security code as follows: The radio and CD player has been replaced.
| Confirm the security code using any of the following methods. Use the security code indicated on the cards retained in the vehicle.
| If the security code is unknown owing to the owner's loss of the card: Remove the radio and CD player referring to . Read the serial number stamped on the radio and CD player. Look up the security code (anti-theft code table) corresponding to the serial number.
| When the radio and CD player is replaced: Use the security code on the cards attached to the upper surface of the replacement radio and CD player. NOTE: Deliver the two cards to the owner. Connect the radio to the vehicle harness. Turn the ignition key to the "ACC" or "ON" position.
| Press the "PWR" button, and "CODE" will be displayed.
| Press number 1 through number 4 memory select button to set the four-digit security code shown on the card. Every time each digit key is pressed, the figure changes as follows: 0 to 1 to 2 to 3 to 4 to 5 to 6 to 7 to 8 to 9 to 0 Press the "CD" button, and a beep will be heard. If entered correctly, the radio and tape player will work. If the security code is not accepted, "1Err" is displayed. In a few seconds, it will change to "CODE." Then repeat steps 5 and 6. NOTE: The anti-theft system will allow three attempts maximum to input the correct code. The second error is displayed as "2 Err." When the third error is made, "3 Err" is displayed and then the display changes to "OFF." If this should occur, the unit will not work any more. To input the security code again, turn the ignition switch to the "ACC" or "ON" position and wait for one hour when "OFF" is displayed. After "OFF" disappears on the display and changes into "CODE" the security code can be input again.
| Three-minute operation mode
| To facilitate replacement or check, the radio with tape and CD player can be operated for three minutes without inputting the security code. Press the "PWR" button and "EJECT" button together to operate the radio with tape and CD player. In three minutes the unit will not be able to work. Then the radio with tape and CD player will be switched off.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - ON-VEHICLE SERVICE - PROCEDURE FOR INPUT OF SECURITY CODE FOR ANTI-THEFT SYSTEM <Vehicles for Australia and New zealand> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation