[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - INVECS-II CANCEL COMMAND | PRINT PAGE / INDEX / PRIOR / NEXT

INVECS-II CANCEL COMMAND
Item No. | Item | Contents | NOTE
--- | --- | --- | ---
14 | INVECS-II | Stop the INVECS-II control and changes gear according to the standard shift pattern. | Use this procedure when carrying out road test procedure 8. If the ignition switch is turned from OFF to ON to OFF, this function restores the INVECS-II control.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - INVECS-II CANCEL COMMAND | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation