[55B] AUTOMATIC AIR CONDITIONER - - PHOTO SENSOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

PHOTO SENSOR

| REMOVAL AND INSTALLATION
|  |  | Disassembly steps
--- | --- | --- | ---
|  | • | Instrument lower panel removal (Refer to GROUP 52A, Instrumental Panel ).
<<A>> | >>A<< | 1. | Photo sensor
| REMOVAL SERVICE POINTS
| <<A>> PHOTO SENSOR REMOVAL
| Binding the photo sensor connector with a cord and rapping a tape around the connector as its surface is flatly to pull out the photo sensor toward the instrument panel upper.
| INSTALLATION SERVICE POINTS
| >>A<< PHOTO SENSOR INSTALLATION
| Tape the photo sensor under the defroster nozzle.

[55B] AUTOMATIC AIR CONDITIONER - - PHOTO SENSOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation