[55A] HEATER, AIR CONDITIONER AND VENTILATION - - BLOWER ASSEMBLY AND RESISTOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

BLOWER ASSEMBLY AND RESISTOR

REMOVAL AND INSTALLATION
|  |  | Blower motor removal step
--- | --- | --- | ---
|  | 1. | Blower motor
|  |  | Resistor removal step
|  | • | Glove box (Refer to GROUP 52A, Instrument Panel <L.H.drive vehicles> or <R.H.drive vehicles>).
|  | 2. | Resistor
|  |  | Outside/inside air selection damper control motor removal step
|  | • | Glove box (Refer to GROUP 52A, Instrument Panel <L.H.drive vehicles> or <R.H.drive vehicles>).
|  | 3. | Outside/inside air selection damper control motor

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - BLOWER ASSEMBLY AND RESISTOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation