[16] ENGINE ELECTRICAL - - STARTING SYSTEM - STARTER MOTOR ASSEMBLY - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G63-DOHC>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Front exhaust pipe connecting bolts
|  | 2. | Starter cover
|  | 3. | Starter connector
<<A>> |  | 4. | Starter assembly
| REMOVAL SERVICE POINT
| <<A>> STARTER ASSEMBLY REMOVAL
| Move the front exhaust pipe to one side to create sufficient clearance for the starter removal. Remove the starter assembly from underneath the vehicle.

[16] ENGINE ELECTRICAL - - STARTING SYSTEM - STARTER MOTOR ASSEMBLY - REMOVAL AND INSTALLATION <4G63-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation