[42] BODY - - DOOR - ON-VEHICLE SERVICE - DOOR WINDOW GLASS ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| DOOR WINDOW GLASS ADJUSTMENT
| Check that the door glass moves while contacting the door glass channel when it is raised and lowered fully. If not, adjust the door window according to the following procedures. Remove the door trim assembly (Refer to GROUP 52A, Door trim ). Remove the waterproof film (Refer to ).
| Loosen the door glass mounting screw via the adjusting hole with the door window glass fully closed, then lower the window glass a little. Fully close the door window glass again and tighten the door glass mounting screw firmly via the adjusting hole.

[42] BODY - - DOOR - ON-VEHICLE SERVICE - DOOR WINDOW GLASS ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation