[55B] AUTOMATIC AIR CONDITIONER - - OTHER PARTS - OTHER PARTS | PRINT PAGE / INDEX / PRIOR / NEXT

OTHER PARTS

| OTHER PARTS The following maintenance service points are the same as for the manual A/C.
Item | Reference page
--- | ---
On-vehicle service | Refrigerant level test |
Magnetic clutch test |
Compressor drive belt adjustment |
A/C pressure sensor simple check |
Charging |
Correcting low refrigerant level in case the service can in used |
Discharging system |
Refilling of oil in the A/C system |
Performance test |
Refrigerant leak repair procedure |
Compressor noise check |
Power relay continuity check |
Idle-up operation check |
Clean air filter replacement procedure |
Blower assembly |
Blower motor and outside/inside air selection damper control motor |
Condenser and condenser fan motor <Vehicles for South Africa> |
Refrigerant line |
Ducts |

[55B] AUTOMATIC AIR CONDITIONER - - OTHER PARTS - OTHER PARTS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation