[55B] AUTOMATIC AIR CONDITIONER - - COMPRESSOR ASSEMBLY AND TENSION PULLEY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| COOLING TEMPRATURE SWITCH CAUTION Do not heat more than necessary.
| Dip the metal part of the cooling temperature switch into engine oil and increase the oil temperature using a gas burner or similar.
| When the oil temperature reaches the standard value, check that voltage is supplied between the terminals. Standard value: <Vehicles for Hong Kong>
Item | Temperature
Less than 2 ohms | Slightly below 150°C
No continuity | 150°C or more
NOTE: When the oil temperature is 150°C or more and there is no continuity, the resistance will not be 2Ω or lower until the oil temperature reduces to 120°C or less. <Vehicles for South Africa>
Item | Temperature
Less than 2 ohms | Slightly below 155°C
No continuity | 155°C or more
NOTE: When the oil temperature is 155°C or more and there is no continuity, the resistance will not be 2Ω or lower until the oil temperature reduces to 125°C or less.

[55B] AUTOMATIC AIR CONDITIONER - - COMPRESSOR ASSEMBLY AND TENSION PULLEY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation