[51] EXTERIOR - - REAR WIPER AND WASHER - ON-VEHICLE SERVICE - CHECK OF REAR WIPER OPERATION WHEN SELECTOR LEVER IS AT THE "R" POSITION | PRINT PAGE / INDEX / PRIOR / NEXT

| ON-VEHICLE SERVICE

| CHECK OF REAR WIPER OPERATION WHEN SELECTOR LEVER IS AT THE "R" POSITION When the selector lever is moved to the "R" position with the rear wiper switch at the "INT" position, the wiper should operate twice or three times at low speed after approximately one second. If not, troubleshoot. (Refer to GROUP 54B, Troubleshooting or GROUP 54C, Troubleshooting or GROUP 54D, Troubleshooting or GROUP 54E, Troubleshooting .)

[51] EXTERIOR - - REAR WIPER AND WASHER - ON-VEHICLE SERVICE - CHECK OF REAR WIPER OPERATION WHEN SELECTOR LEVER IS AT THE "R" POSITION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation