[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - TROUBLESHOOTING - SYMPTOM PROCEDURES - Inspection Procedure 17: Run on (Dieseling) | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection Procedure 17: Run on (Dieseling)
COMMENT ON TROUBLE SYMPTOM Failure is possibly caused by leakage from injector.
PROBABLE CAUSE Failed injector Failed engine-A/T-ECU
| DIAGNOSIS PROCEDURE
| STEP 1. Check injector for spray condition. Check each injector for spray condition (Refer to ). Q: Does trouble symptom persist? YES: Replace engine-A/T-ECU. NO: Replace injector.

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - TROUBLESHOOTING - SYMPTOM PROCEDURES - Inspection Procedure 17: Run on (Dieseling) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation