[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B2. CHECK SUSPENSION ARM BALL JOINTS FOR PLAY, AND DUST COVERS FOR DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

| B2. CHECK SUSPENSION ARM BALL JOINTS FOR PLAY, AND DUST COVERS FOR DAMAGE
| LOWER ARM BALL JOINT END PLAY CHECK
| Raise the vehicle. Remove the stabilizer bar from the lower arm assembly. Move the lower arm up and down with your hands to check for an excessive play in the axial direction of the ball joint. If there is an excessive play, replace the lower arm assembly.
| DUST COVERS FOR DAMAGE Check dust covers for damage.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B2. CHECK SUSPENSION ARM BALL JOINTS FOR PLAY, AND DUST COVERS FOR DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation