[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - REMOVAL AND DISASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

| REMOVAL AND DISASSEMBLY
| When checking a malfunction, find the cause of the problem. If it is determined that removal and/or disassembly is necessary, perform the work by following the procedures contained in this manual.
| If punch marks or mating marks are made to avoid error in assembly and facilitate the assembly work, be sure to make them in locations which will have no detrimental effect on performance and/or appearance. If an area having many parts, similar parts, and/or parts which are symmetrical right and left is disassembled, be sure to arrange the parts so that they do not become mixed during the assembly process. Arrange the parts removed in the proper order. Determine which parts are to be reused and which are to be replaced. If bolts, nuts, etc., are to be replaced, be sure to use only the exact size specified.

[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - REMOVAL AND DISASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation