[33] FRONT SUSPENSION - - LOWER ARM - LOWER ARM REAR BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| LOWER ARM REAR BUSHING REPLACEMENT
| Replace the bushing as follows:
| Use following special tools to drive out the bushing. MB990883: Rear Suspension Bushing Arbor MB990972: Torsion Bar Bushing Remover Base MB990887: Ring MB990890: Rear Suspension Bushing Base
| Position the bushing so that its projection is as shown, and then use the special tools to press in the bushing. Press the bushing until its outer tube is flush with the lower arm assembly surface.

[33] FRONT SUSPENSION - - LOWER ARM - LOWER ARM REAR BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation