[27A] REAR AXLE <2WD> - - ON-VEHICLE SERVICE - REAR HUB ROTARY-SLIDING RESISTANCE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| REAR HUB ROTARY-SLIDING RESISTANCE CHECK Remove the brake drum. Turn the hub a few times to seat the bearing.
| Wind a rope around the hub bolt and turn the hub by pulling at a 90° angle with a spring balance. Measure to determine whether or not the rotary-sliding resistance of the rear hub is at the limit value. Limit: 19 N If limit value is exceeded, loosen the self-locking nut and then tighten it to the specified torque and check the rear hub rotary sliding resistance again. Tightening torque: 175 ± 25 N·m Replace the rear hub assembly if an adjustment cannot be made to within the limit.

[27A] REAR AXLE <2WD> - - ON-VEHICLE SERVICE - REAR HUB ROTARY-SLIDING RESISTANCE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation