[32] POWER PLANT MOUNT - - ENGINE MOUNTING - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ENGINE MOUNTING

REMOVAL AND INSTALLATION
<SOHC> CAUTION *: Indicates parts which should be initially tightened, and then fully tightened after placing the vehicle horizontally and loading the full weight of the engine on the vehicle body.
Pre-removal Operation Raise the engine and transmission assembly until its weight is not applied to the insulator, and support it securely.
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Pressure hose clamp
|  | 2. | Self-locking nut
|  | 3. | Engine front mounting bracket
<DOHC> CAUTION *: Indicates parts which should be initially tightened, and then fully tightened after placing the vehicle horizontally and loading the full weight of the engine on the vehicle body.
Pre-removal Operation Raise the engine and transmission assembly until its weight is not applied to the insulator, and support it securely. Reserve Tank Removal (Refer to GROUP 14, Radiator ). | Post-installation Operation Reserve Tank Installation (Refer to GROUP 14, Radiator ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Pressure hose clamp
|  | 2. | Self-locking nut
|  | 3. | Engine mounting adapter
| >>A<< | 4. | Engine mounting stopper
|  | 5. | Engine mounting
| INSTALLATION SERVICE POINT
| >>A<< ENGINE MOUNTING STOPPER INSTALLATION
| Install the engine mounting stopper so that its arrow faces towards the engine.

[32] POWER PLANT MOUNT - - ENGINE MOUNTING - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation