[52A] INTERIOR - - FRONT SEAT BELT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| SEAT BELT BUCKLE SWITCH CONTINUITY CHECK
Items | Tester connection | Specified condition
--- | --- | ---
Fastened seat belt | 1 - 2 | Open circuit
Unfastened seat belt | 1 - 2 | Less than 2 ohms

[52A] INTERIOR - - FRONT SEAT BELT - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation