[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-4: Front and/or rear passenger's power window(s) do not work by means of the power window main switch. <LH drive vehicles except for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE D-4: Front and/or rear passenger's power window(s) do not work by means of the power window main switch. <LH drive vehicles except for Argentina>
| COMMENTS ON TROUBLE SYMPTOM If the passenger's and/or rear power window does not work by means of the power window main switch, the power window main switch or the respective power window sub switch(es) may be defective.
| POSSIBLE CAUSES Malfunction of the power window main switch Malfunction of the power window sub switch (front RH), power window sub switch (rear RH) or power window sub switch (rear LH) Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check the power window main switch. Check that the driver's power window works by means of the power window main switch. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to Inspection Procedure D-2 "Driver's power window does not work by means of the power window main switch <Except vehicles for Argentina> ."
| Step 2. Check the power window sub switch. Check that each power window works by means of the respective power window sub switch when the power window lock switch is turned off. Q: Is the check result normal? YES: Go to Step 3. NO: Refer to Inspection Procedure D-3 "Relevant power window(s) do not work by means of the front and rear passenger's power window sub switches <LH drive vehicles except for Argentina> ."
| Step 3. Connector check: E-05 power window main switch connector Q: Is the check result normal? YES: Go to Step 4. NO: Repair the connector.
| Step 4. Check the power window main switch. Refer to GROUP 42 - Door . Q: Is the check result normal? YES: Go to Step 5. NO: Replace the power window main switch.
| Step 5. Determine a trouble spot. Q: Which power window does not work when the power window main switch is operated? Front passenger's door: Go to Step 6. Rear right door: Go to Step 9. Rear left door: Go to Step 12.
| Step 6. Connector check: E-17 power window sub switch (front RH) connector Q: Is the check result normal? YES: Go to Step 7. NO: Repair the connector.
| Step 7. Check the power window sub switch (front RH). Refer to GROUP 42 - Door . Q: Is the check result normal? YES: Go to Step 8. NO: Replace the power window sub switch (front RH).
| Step 8. Check the wiring harness from E-17 power window sub switch (front RH) connector terminals 4 and 8 to E-05 power window main switch connector terminals 3 and 11. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-15, C-118, E-12 and E-24, and repair if necessary. Check the power window operating lines for open or short circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 9. Connector check: E-21 power window sub switch (rear RH) connector Q: Is the check result normal? YES: Go to Step 10. NO: Repair the connector.
| Step 10. Check the power window sub switch (rear RH). Refer to GROUP 42 - Door . Q: Is the check result normal? YES: Go to Step 11. NO: Replace the power window sub switch (rear RH).
| Step 11. Check the wiring harness from E-21 power window sub switch (rear RH) connector terminals 4 and 8 to E-05 power window main switch connector terminals 14 and 6. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-13, C-118, D-01, E-12 and E-27, and repair if necessary. Check the power window operating lines for open or short circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 12. Connector check: E-01 power window sub switch (rear LH) connector Q: Is the check result normal? YES: Go to Step 13. NO: Repair the connector.
| Step 13. Check the power window sub switch (rear LH). Refer to GROUP 42 - Door . Q: Is the check result normal? YES: Go to Step 14. NO: Replace the power window sub switch (rear LH).
| Step 14. Check the wiring harness from E-21 power window sub switch (rear LH) connector terminals 4 and 8 to E-05 power window main switch connector terminals 1 and 2. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-117, C-118, D-25, E-09 and E-12, and repair if necessary. Check the power window operating lines for open or short circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - POWER WINDOWS - INSPECTION PROCEDURE D-4: Front and/or rear passenger's power window(s) do not work by means of the power window main switch. <LH drive vehicles except for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation