[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - COMBINATION METER ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

COMBINATION METER ASSEMBLY

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Instrument panel driver’s side garnish (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 2. | Meter bezel (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 3. | Combination meter assembly

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - COMBINATION METER ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation