[55B] AUTOMATIC AIR CONDITIONER - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
Idle speed r/min | 2000 SOHC | 750 ± 100
2000 DOHC | 750 ± 100
2400 | 700 ± 100
Idle-up speed r/min | 2000 SOHC | 850 ± 100
2000 DOHC | 800 ± 100
2400 | 850 ± 100
Resistance value for air mixing door control motor and potentiometer kΩ | MAX HOT | Approximately 5.35
MAX COOL | Approximately 0.65
Resistance value for mode selection damper control motor and potentiometer kΩ | DEF position | Approximately 0.65
FACE position | Approximately 5.35

[55B] AUTOMATIC AIR CONDITIONER - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation