[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - KEYLESS ENTRY SYSTEM - INSPECTION PROCEDURE E-7: The timer lock function does not work after the doors have been unlocked by the keyless entry system. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE E-7: The timer lock function does not work after the doors have been unlocked by the keyless entry system.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If the keyless entry timer lock does not work normally, the input signal circuit(s) to the keyless entry transmitter or the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the keyless entry transmitter Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check the operation of the keyless entry system. Check that the keyless entry system works normally. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to inspection procedure E-1 "Keyless entry system does not work ."
| Step 2. Retest the system. Check that the timer lock works normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - KEYLESS ENTRY SYSTEM - INSPECTION PROCEDURE E-7: The timer lock function does not work after the doors have been unlocked by the keyless entry system. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation