[12] ENGINE LUBRICATION - - ON-VEHICLE SERVICE - ENGINE OIL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

ON-VEHICLE SERVICE

| ENGINE OIL CHECK Pull out the level gauge slowly and check that the oil level is in the illustrated range. Check that the oil is not excessively dirty, that there is no coolant or petrol mixed in, and that it has sufficient viscosity.

[12] ENGINE LUBRICATION - - ON-VEHICLE SERVICE - ENGINE OIL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation