[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLESHOOTING - DATA LIST CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

DATA LIST CHECK
Use the MUT-II/III and the SWS monitor to check "DATA LIST." This "DATA LIST" check is applicable for signals, which are transmitted and received through the SWS communication line and the communication lines routed from one door to another. For the input signals which are not applicable for the SWS monitor check, refer to pulse check procedure . NOTE: If a problem is found in the "DATA LIST" check, refer to the Problems during Input Signal Check <Service data, function diagnosis or pulse check> (Refer to ). The following input signals can be checked by using the MUT-II/III and the SWS monitor.
DATA LIST REFERENCE TABLE
| COLUMN SWITCH (COLUMN-ECU)
Item No. | Check item | Display on MUT-II/III | Check condition | Normal condition
--- | --- | --- | --- | ---
00 | Headlamp switch | HEADLAMP SW | Lighting switch: HEAD | ON
Lighting switch: Other than HEAD | OFF
01 | Tail lamp switch | TAIL LAMP SW | Lighting switch: TAIL | ON
Lighting switch: OFF | OFF
02 | Dimmer switch | DIMMER SW | Dimmer switch: ON | ON
Dimmer switch: OFF | OFF
03 | Passing lamp switch | PASSING SW | Passing lamp which: ON | ON
Passing lamp which: OFF | OFF
05 | Windshield intermittent wiper switch | INT WIPER SW | Wiper switch: INT | ON
Wiper switch: Other than INT | OFF
06 | Windshield low-speed wiper switch | LO WIPER SW | Wiper switch: LO | ON
Wiper switch: Other than LO | OFF
07 | Windshield high-speed wiper switch | HI WIPER SW | Wiper switch: HI | ON
Wiper switch: Other than HI | OFF
08 | Wind shield mist wiper switch | MIST WIPER SW | Wiper switch: Mist | ON
Wiper switch: Other than mist | OFF
09 | Windshield washer switch | FRONT WASH. SW | Windshield washer switch: ON | ON
Windshield washer switch: OFF | OFF
10 | Turn-signal lamp switch (RH) | TURN SIG. RH | Turn-signal lamp switch: RH | ON
Turn-signal lamp switch: Other than RH | OFF
11 | Turn-signal lamp switch (LH) | TURN SIG. LH | Turn-signal lamp switch: LH | ON
Turn-signal lamp switch: Other than LH | OFF
13 | Rear wiper switch | REAR WIPER SW | Rear wiper switch: INT | ON
Rear wiper switch: Other than INT | OFF
14 | Rear washer switch | REAR WASH. SW | Rear wiper switch: Washer | ON
Rear wiper switch: Other than washer | OFF
15 | With or without windshield intermittent wiper control | INT WIP KNOB | Vehicles with intermittent wiper control | EQUIP
Vehicles without intermittent wiper control | NONE
| ETACS-ECU
Item No. | Check item | Display on MUT-II/III | Check condition | Normal condition
--- | --- | --- | --- | ---
30 | Ignition switch (IG1) | IG SW(IG1) | Ignition switch: ON or START | ON
Ignition switch: LOCK (OFF) or ACC | OFF
31 | Ignition switch (ACC) | IG SW(ACC) | Ignition switch: ACC or ON | ON
Ignition switch: LOCK (OFF) or START | OFF
32 | Driver's door switch*1 | DR DOOR SW | Driver's door switch ON (The driver’s door is open). | ON
Driver's door switch OFF (The driver's door is closed). | OFF
Front door switch*2 | FRONT DOOR SW | Front door switch: ON (front door open) | ON
Front door switch: OFF (front door closed) | OFF
33 | Reception of power window switch | P/W SW ACCEPT | Ignition switch: ON or START | PERMIT
Ignition switch: from ON or START to LOCK (OFF) or ACC | from PERMIT to PROHIBIT (after approximately 30 seconds)
34 | Multimode keyless entry system | KEYLESS ENTRY | Keyless entry transmitter LOCK switch: ON Turn ON the keyless entry transmitter LOCK switch again (For the second switch operation, hold pressing the switch for at least one second within 30 seconds after the switch is turned on at first) | MULTI CLOSE (only momentarily when switch is operated)
Keyless entry transmitter UNLOCK switch: ON Turn ON the keyless entry transmitter UNLOCK switch again (For the second switch operation, hold pressing the switch for at least one second within 30 seconds after the switch is turned on at first) | MULTI OPEN (only momentarily when switch is operated)
When multimode is working Turn on any function of the keyless entry transmitter again. | MULTI STOP (only momentarily when switch is operated)
Other than the conditions above | WAITING
35 | Headlamp automatic shutdown function | HD AUTO-CUT | Lighting switch: Other than OFF Ignition switch: from ON or START to LOCK (OFF) or ACC Driver's door switch: ON (driver's door open) | OFF to ON (after approximately one second)
When requirements for the headlamp automatic shutdown are not satisfied | OFF
36 | Request of fog lamp illumination | F.FOG LAMP | Lighting switch: "TAIL" or "HEAD" Fog lamp switch: ON | ON
Other than the conditions above | OFF
37 | Windshield intermittent wiper interval | INT WIPE TIME | Ignition switch: ACC or ON Operate the intermittent wiper control, and change the wiper interval | The MUT-II/III displays intermittent wiper interval in response to the intermittent wiper control positions
41 | Park/neutral switch ("R" position) | INHIBITOR SW | Park/neutral switch: "R" position | ON
Park/neutral switch: Other than "R" position | OFF
43 | Buzzer | BUZZER | Ignition switch: LOCK (OFF) Key reminder switch: ON Driver's door switch: ON (driver's door open) | ON
When requirements for sounding each warning buzzer are not satisfied | OFF
| NOTE: For item number 43, the MUT-II/III also displays "ON" when the lamp reminder buzzer or R (reverse) position warning buzzer is triggered. *1 : Except for Australia *2 : Vehicles for Australia
| FRONT-ECU
Item No. | Check item | Display on MUT-II/III | Check condition | Normal condition
--- | --- | --- | --- | ---
70 | Response by the front-ECU | Front ECU response | Lighting switch: Other than OFF (excluding when high-beam is on) or the wiper switch is at position other than OFF | Normal response
Ignition switch: ON or START Lighting switch: OFF Wiper switch: OFF | SLEEP RESPONSE
Lighting switch: HEAD Headlamps: at high beam | HI BEAM RESPONSE
- | No response
| NOTE: For item number 70, the MUT-II/III also displays "NG" under the "ECU Check" when it displays "No response" under the front-ECU check.
| POWER WINDOW MAIN SWITCH (POWER WINDOW MODULE) <VEHICLES FOR ARGENTINA ONLY>
Item No. | Check item | Display on MUT-II/III | Check condition | Normal condition
--- | --- | --- | --- | ---
71 | Response from power window module | P/W ECU ACK | Ignition switch: ON or START | NORMAL ACK
Ignition switch: ON or START Operate any switch of the power window main switch. | INPUT CHECK (only momentarily when switch is operated)
- | NO ACK
| NOTE: For item number 71, the MUT-II/III also displays "NG" under the "ECU CHECK" when it displays "NO ACK" under the "P/W ECU ACK" check.
| SUNROOF MOTOR ASSEMBLY (SUNROOF-ECU)
Item No. | Check item | Display on MUT-II/III | Check condition | Normal condition
--- | --- | --- | --- | ---
72 | Response by the sunroof-ECU | S/R ECU ACK | Ignition switch: ON or START While sunroof is off | NORMAL ACK → SLEEP ACK (after approximately 30 seconds)
Ignition switch: ON or START One of the sunroof switches is on | INPUT CHECK → NORMAL ACK
- | NO ACK
| NOTE: For item number 72, the MUT-II/III also displays "NG" under the "ECU CHECK" when it displays "NO ACK" under the "S/R ECU ACK" check.
FUNCTION DIAGNOSIS The table below shows the service data and their normal condition, which are displayed during the "FUNCTION DIAG." The row "Normal conditions" shows values, which are shown when each operation is made.
| WIPER
ITEM | Input signal | Item No. | Display on MUT-II/III | Normal condition
--- | --- | --- | --- | ---
F.WIPER INT (intermittent) | Windshield intermittent wiper switch | 05 | INT WIPER SW | ON
Windshield low-speed wiper switch | 06 | LO WIPER SW | OFF
Windshield high-speed wiper switch | 07 | HI WIPER SW | OFF
Wind shield mist wiper switch | 08 | MIST WIPER SW | OFF
Windshield washer switch | 09 | FRONT WASH. SW | OFF
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
Windshield intermittent wiper interval | 37 | WIPER INT TIME | The MUT-II/III displays intermittent wiper interval in response to the intermittent wiper control positions
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
F.WIPER LO (low speed) | Windshield intermittent wiper switch | 05 | INT WIPER SW | OFF
Windshield low-speed wiper switch | 06 | LO WIPER SW | ON
Windshield high-speed wiper switch | 07 | HI WIPER SW | OFF
Wind shield mist wiper switch | 08 | MIST WIPER SW | OFF
Windshield washer switch | 09 | FRONT WASH. SW | OFF
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
F.WIPER HI (high speed) | Windshield intermittent wiper switch | 05 | INT WIPER SW | OFF
Windshield low-speed wiper switch | 06 | LO WIPER SW | OFF
Windshield high-speed wiper switch | 07 | HI WIPER SW | ON
Wind shield mist wiper switch | 08 | MIST WIPER SW | OFF
Windshield washer switch | 09 | FRONT WASH. SW | OFF
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
F.WIPER MIST | Windshield intermittent wiper switch | 05 | INT WIPER SW | OFF
Windshield low-speed wiper switch | 06 | LO WIPER SW | OFF
Windshield high-speed wiper switch | 07 | HI WIPER SW | OFF
Wind shield mist wiper switch | 08 | MIST WIPER SW | ON
Windshield washer switch | 09 | FRONT WASH. SW | OFF
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
F.WIPER WASH | Wind shield mist wiper switch | 08 | MIST WIPER SW | OFF
Windshield washer switch | 09 | FRONT WASH. SW | ON
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
| REAR WIPER
ITEM | Input signal | Item No. | Display on MUT-II/III | Normal condition
--- | --- | --- | --- | ---
REAR WIPER | Rear wiper switch | 13 | REAR WIPER SW | ON
Rear washer switch | 14 | REAR WASH. SW | OFF
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
REV. INTERLOCK | Rear wiper switch | 13 | REAR WIPER SW | ON
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
Park/neutral switch ("R" position) | 41 | INHIBITOR SW | ON
REAR WASHER | Rear washer switch | 14 | REAR WASH. SW | ON
Ignition switch (ACC) | 31 | IG SW(ACC) | ON
| LIGHTING
ITEM | Input signal | Item No. | Display on MUT-II/III | Normal condition
--- | --- | --- | --- | ---
OFF | Headlamp switch | 00 | HEADLAMP SW | OFF
Tail lamp switch | 01 | TAIL LAMP SW | OFF
Passing lamp switch | 03 | PASSING SW | OFF
Ignition switch (IG1)* | 30 | IG SW(IG1) | ON
Headlamp automatic shutdown function* | 35 | HD AUTO-CUT | OFF
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
TAIL LAMP | Headlamp switch | 00 | HEADLAMP SW | OFF
Tail lamp switch | 01 | TAIL LAMP SW | ON
Passing lamp switch | 03 | PASSING SW | OFF
Ignition switch (IG1)* | 30 | IG SW(IG1) | ON
Headlamp automatic shutdown function* | 35 | HD AUTO-CUT | OFF
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK
HEADLAMP LO (low-beam) | Headlamp switch | 00 | HEADLAMP SW | ON
Passing lamp switch | 03 | PASSING SW | OFF
Ignition switch (IG1)* | 30 | IG SW(IG1) | ON
Headlamp automatic shutdown function* | 35 | HD AUTO-CUT | OFF
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK
HEADLAMP HI (high-beam) | Headlamp switch | 00 | HEADLAMP SW | ON
Dimmer switch | 02 | DIMMER SW | ON
Ignition switch (IG1)* | 30 | IG SW(IG1) | ON
Headlamp automatic shutdown function* | 35 | HD AUTO-CUT | OFF
Response by the front-ECU | 70 | FRONT ECU ACK | HI-BEAM ACK
PASSING LAMP | Passing lamp switch | 03 | PASSING SW | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
F.FOG LAMP | Headlamp switch | 00 | HEADLAMP SW | Either of items is ON
Tail lamp switch | 01 | TAIL LAMP SW
Ignition switch (IG1)* | 30 | IG SW(IG1) | ON
Headlamp automatic shutdown function* | 35 | HD AUTO-CUT | OFF
Request of fog lamp illumination | 36 | F.FOG LAMP | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK
REAR FOG LAMP | Headlamp switch | 00 | HEADLAMP SW | ON
Tail lamp switch | 01 | TAIL LAMP SW | ON
Headlamp automatic shutdown function* | 35 | HD AUTO-CUT | OFF
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
HD AUTO-CUT* | Headlamp switch | 00 | HEADLAMP SW | Either is on
Tail lamp switch | 01 | TAIL LAMP SW
Ignition switch (IG1) | 30 | IG SW(IG1) | OFF
Driver's door switch | 32 | DR DOOR SW | ON
Headlamp automatic shutdown function | 35 | HD AUTO-CUT | ON
Response by the front-ECU | 70 | FRONT ECU ACK | NORMAL ACK or HI-BEAM ACK
| NOTE: When checking the input signals (off, tail, low-beam or high-beam), turn the ignition switch to the "ON" position in order to disable the headlamp automatic shutdown function. However, the titles on the MUT-II/III screen will not be highlighted as this has nothing to do with actual lamp operation. For checking item "HEADLAMP HI", the MUT-II/III displays "OFF" on the item No.02 "DIMMER SW" when the headlamps are at high-beam. Therefore, the MUT-II/III should display "ON" momentarily when the dimmer switch is operated. * : Except for Australia
| TURN-SIGNAL LAMP
ITEM | Input signal | Item No. | Display on MUT-II/III | Normal condition
--- | --- | --- | --- | ---
Turn-signal lamp (RH) | Turn-signal lamp switch (RH) | 10 | TURN SIGNAL RH SW | ON
Turn-signal lamp switch (LH) | 11 | TURN SIGNAL LH SW | OFF
Ignition switch (IG1) | 30 | IGNITION SW IG1 | ON
Turn-signal lamp (LH) | Turn-signal lamp switch (RH) | 10 | TURN SIGNAL RH SW | OFF
Turn-signal lamp switch (LH) | 11 | TURN SIGNAL LH SW | ON
Ignition switch (IG1) | 30 | IGNITION SW IG1 | ON
| BUZZER
ITEM | Input signal | Item No. | Display on MUT-II/III | Normal condition
--- | --- | --- | --- | ---
Lighting monitor buzzer | Headlamp switch | 00 | HEADLAMP SW | Either is on
Tail lamp switch | 01 | TAIL LAMP SW
Ignition switch (IG1) | 30 | IGNITION SW IG1 | OFF
Driver's door switch | 32 | DRIVER DOOR SW | ON
Headlamp automatic shutdown function | 35 | HD LAMP AUTOCUT | OFF
Buzzer | 43 | BUZZER | ON
Key reminder buzzer* | Ignition switch (IG1) | 30 | IGNITION SW IG1 | OFF
Driver's door switch | 32 | DRIVER DOOR SW | ON
Buzzer | 43 | BUZZER | ON
| NOTE: The headlamp automatic shutdown function works in approximately one second after the lighting monitor buzzer starts sounding, and then the buzzer ceases sounding. * : Except for Australia
| SUNROOF
ITEM | Input signal | Item No. | Display on MUT-II/III | Normal condition
--- | --- | --- | --- | ---
SUNROOF OPE. | Ignition switch (IG1) | 30 | IG SW(IG1) | ON
Response by power window module | 71 | P/W ECU ACK | NORMAL ACK
Response by the sunroof-ECU | 72 | S/R ECU ACK | INPUT CHECK (only momentarily when switch is operated)

[54E] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLESHOOTING - DATA LIST CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation