[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - VACUUM HOSE - VACUUM HOSE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| VACUUM HOSE CHECK Using the piping diagram as a guide, check to be sure that the vacuum hoses are correctly connected. Check the connection condition of the vacuum hoses, (removed, loose, etc.) and check to be sure that there are no bends or damage.

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - VACUUM HOSE - VACUUM HOSE CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation