[34] REAR SUSPENSION - - GENERAL DESCRIPTION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL DESCRIPTION
A trailing arm type multi-link suspension has been adopted as the rear suspension. The shock absorber is a hydraulic, cylindrical double-acting type.
CONSTRUCTION DIAGRAM
SPECIFICATION
COIL SPRING
Item | 2000 | 2400
--- | --- | ---
SOHC | DOHC | Vehicles for General Export, GCC, Brazil, Australia and New Zealand | Vehicles for Hong Kong spec. | Vehicles for South Africa and Argentina
Wire diameter mm | 10 | 11 | 11 | 11 | 11
Average diameter mm | 90 | 91 | 91 | 91 | 91
Free length mm | 368 | 333 | 380 | 373 | 350

[34] REAR SUSPENSION - - GENERAL DESCRIPTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation