[3] WELDED PANEL REPLACEMENT - - ROOF | PRINT PAGE / INDEX / PRIOR / NEXT

ROOF
Adhesive 1 : Urethane body sealer Brand : 3M ATD Part No.8542 or equivalent Adhesive 2 : Epoxyayresin adhesive Brand : 3M ATD Part No.8115 or equivalent Adhesive 1 : Urethane body sealer Brand : 3M ATD Part No.8542 or equivalent Adhesive 2 : Epoxyayresin adhesive Brand : 3M ATD Part No.8115 or equivalent
| NOTE ON REPAIR WORK
| REMOVAL
| The welding point is at the bottom of the roof rack bracket rear. Thus, remove the roof rack bracket rear and detach the welding point.
| INSTALLATION
| When assembling the roof panel, apply in advance adhesive to the areas shown in the figure of the instructions. Adhesive : Epoxyayresin adhesive Brand : 3M ATD Part No.8115 or equivalent Remove the roof rack bracket rear from the new parts. Weld the roof panel. Then assemble the roof rack bracket rear.

[3] WELDED PANEL REPLACEMENT - - ROOF | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation