[4] CORROSION PROTECTION - - BODY SEALING LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

BODY SEALING LOCATIONS
If the sealant application is directly visible on the outer plate and requires appearance quality of the application in areas such as the drip rail, pillar, clinch and so on, then apply the sealant so that it is flat, or wipe off any excess mounding after the application. Be careful not to obstruct the water draining hole. NOTE: The bold dotted line indicates the application area on the underside.
FLOOR
UPPER BODY
SIDE BODY

[4] CORROSION PROTECTION - - BODY SEALING LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation