[54B] SMART WIRING SYSTEM (SWS) - - COMMUNICATION METHOD | PRINT PAGE / INDEX / PRIOR / NEXT

COMMUNICATION METHOD The exclusive signal lines for transmitting the multi-distribution data are connected as follows between the ETACS-ECU, column switch (incorporated inside the column-ECU), front-ECU, sunroof motor assembly (incorporated inside the sunroof-ECU), power window main switch (incorporated inside the power window-ECU), and power window sub switches (incorporated inside the power window-ECU) <Vehicles for Hong Kong spec. and Argentina> for internal communication.

[54B] SMART WIRING SYSTEM (SWS) - - COMMUNICATION METHOD | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation