[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A12. CHECK AIR CLEANER ELEMENT FOR CLOGGING AND DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

| A12. CHECK AIR CLEANER ELEMENT FOR CLOGGING AND DAMAGE
| Check air cleaner element for clogging and damage. Clean deposited dust from the element in the following manner. Lightly tap the element against the top of a bench. Blow compressed air from inside the element. Wipe off dust on the air cleaner interior. Install the air cleaner body.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A12. CHECK AIR CLEANER ELEMENT FOR CLOGGING AND DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation