[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - KEYLESS ENTRY SYSTEM TIMER LOCK FUNCTION INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| KEYLESS ENTRY SYSTEM TIMER LOCK FUNCTION INSPECTION Push the transmitter unlock button and check to see that the doors and tailgate lock within 30 seconds. If it doesn't, then execute troubleshooting remedies. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . NOTE: The adjustment function allows you to change the keyless entry system timer lock period from 30 seconds (initial setting) to 1, 2 or 3 minutes. Prior to the check, confirm which setting is activated. <Vehicles for Hong Kong spec>

[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - KEYLESS ENTRY SYSTEM TIMER LOCK FUNCTION INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation