[11E] ENGINE MECHANICAL <4G69> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Drive belt tension | Vibration frequency Hz (Reference) | Except for Hong Kong spec. | 120 - 154 | -
For Hong Kong spec. | 113 - 145 | -
Tension N (Reference) | 340 - 555 | -
Valve clearance (at hot) mm | Intake valve | 0.20 | -
Exhaust valve | 0.30 | -
Basic ignition timing | 5° BTDC ± 3° | -
Ignition timing | Approximately 10° BTDC | -
Idle speed r/min | 680 ± 100 | -
CO contents % | 0.5 or less | -
HC contents ppm | 100 or less | -
Compression pressure kPa-r/min | 1,560 - 200 | 1,130 - 200
Compression pressure difference of all cylinders kPa | - | Maximum 98
Intake manifold vacuum kPa | - | Minimum 60
Cylinder head bolt nominal length mm | - | 99.4
Balancer timing belt tension (When adjusted) | Deflection mm | 5 - 7 | -
Balancer timing belt tension (When replaced) | Deflection mm | 5 - 7 | -
Balancer timing belt tension (When checked) | Deflection mm | 5 - 10 | -
Timing belt tensioner adjuster rod protrusion amount mm | 3.8 - 4.5 | -
Timing belt tensioner adjuster rod movement mm | Within 1 | -

[11E] ENGINE MECHANICAL <4G69> - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation