[16] ENGINE ELECTRICAL - - STARTING SYSTEM - STARTER MOTOR ASSEMBLY - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G69>
Pre-removal and Post-installation Operation Air Duct Removal and Installation (Refer to GROUP 15, Air Cleaner ). Exhaust Manifold Heat Protector Removal and Installation (Refer to GROUP 15, Exhaust Manifold ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Starter cover
|  | 2. | Harness clamp
|  | 3. | Starter connector
|  | 4. | Starter terminal
<<A>> |  | 5. | Starter assembly
|  | 6. | Starter cover bracket
| REMOVAL SERVICE POINT
| <<A>> STARTER ASSEMBLY REMOVAL Remove the starter assembly from above the vehicle.

[16] ENGINE ELECTRICAL - - STARTING SYSTEM - STARTER MOTOR ASSEMBLY - REMOVAL AND INSTALLATION <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation