[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - GENERAL INFORMATION (EVAPORATIVE EMISSION CONTROL SYSTEM) <4G64> | PRINT PAGE / INDEX / PRIOR / NEXT

| GENERAL INFORMATION (EVAPORATIVE EMISSION CONTROL SYSTEM) <4G64>
| The evaporative emission control system prevents fuel vapours generated in the fuel tank from escaping into the atmosphere. Fuel vapours from the fuel tank flow through the fuel tank pressure control valve and vapour pipe/hose to be stored temporarily in the canister. When driving the vehicle, fuel vapours stored in the canister go into the intake manifold to be sent to the combustion chamber.

[17] ENGINE AND EMISSION CONTROL - - EMISSION CONTROL <MPI> - EVAPORATIVE EMISSION CONTROL SYSTEM - GENERAL INFORMATION (EVAPORATIVE EMISSION CONTROL SYSTEM) <4G64> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation