[27A] REAR AXLE <2WD> - - ON-VEHICLE SERVICE - HUB BOLT REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| HUB BOLT REPLACEMENT Remove the brake drum.
| Use the following special tools to remove the hub bolts. Front hub and flange yoke holder (MB990767) Hub bolt remover (MB991618) NOTE: To retain a space for removing the hub bolts, remove them near the retainer spring mounting position.
| Install the plain washer to the new hub bolt, and install the bolt with a nut.

[27A] REAR AXLE <2WD> - - ON-VEHICLE SERVICE - HUB BOLT REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation