[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - AUTO-CRUISE CONTROL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

AUTO-CRUISE CONTROL

REMOVAL AND INSTALLATION
WARNING Before removal of the air bag module, refer to GROUP 52B, Service Precautions () and Air Bag Module(s) and Clock Spring (). When removing and installing the steering wheel and air bag module assembly, do not let it bump against the air bag module.
|  |  | Auto-cruise control switch removal
--- | --- | --- | ---
|  | • | Auto-cruise control switch (Refer to GROUP 52B, Air Bag Module(s) and Clock Spring )
|  |  | Control unit removal
|  | • | Engine-A/T-ECU (Refer to GROUP 13C, Engine-A/T-ECU )
|  |  | Sensor removal steps
|  | • | Inhibitor switch (Refer to GROUP 23B, Transmission )
|  | • | Accelerator pedal position sensor <L.H. drive vehicles> (Refer to )
|  | • | Accelerator pedal assembly <R.H. drive vehicles> (Refer to )
|  | • | Throttle body assembly (Refer to GROUP 13C, Throttle body assembly )
|  | • | Stop lamp switch (Refer to GROUP 35A, Brake pedal )

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - AUTO-CRUISE CONTROL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation