[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - CHECK CHART FOR TROUBLE SYMPTOMS | PRINT PAGE / INDEX / PRIOR / NEXT

CHECK CHART FOR TROUBLE SYMPTOMS
Trouble symptom | Inspection procedure No. | Reference page
--- | --- | ---
Communication with MUT-II/III is not possible. | Communication with all systems is not possible. | - |
Communication with auto-cruise control-ECU only is not possible. | 1 |
Auto-cruise control is not cancelled. | Even if brake pedal is depressed | 2 |
Even if select lever is set to N range | 3 |
Even if auto-cruise control CANCEL switch in set to ON | 4 |
Auto-cruise control cannot be set. | 5 |
Hunting (repeated acceleration and deceleration) occurs at the set vehicle speed. | 6 |
When the auto-cruise control MAIN switch is turned ON, the auto-cruise control indicator lamp does not illuminate (However, the auto-cruise control system is normal). | 7 |

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - CHECK CHART FOR TROUBLE SYMPTOMS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation