[33] FRONT SUSPENSION - - ON-VEHICLE SERVICE - BALL JOINT DUST COVER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| BALL JOINT DUST COVER CHECK Press the dust cover with your finger to check that there are no cracks or damage in the dust cover. If the dust cover is cracked or damaged, replace the lower arm assembly or stabilizer link. NOTE: If the dust cover is cracked or damaged, it is possible that there may also be damage to the ball joint.

[33] FRONT SUSPENSION - - ON-VEHICLE SERVICE - BALL JOINT DUST COVER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation