[11B] ENGINE OVERHAUL <4G6-SOHC> - - GENERAL SEPCIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL SEPCIFICATIONS
Item | 4G63-SOHC | 4G64-SOHC
--- | --- | ---
Bore × stroke mm | 85 × 88 | 86.5 × 100
Displacement mL | 1,997 | 2,351
Number of cylinders | 4
Valve mechanism | Type | Single overhead camshaft
Number of intake valves | 2
Number of exhaust valves | 2
Lash adjusters | Hydraulic
Rocker arms | Roller rocker arms
Compression ratio | 10.0 | 9.0
Fuel injection system | Electronically controlled multi-point injection system
Ignition system | Electronically controlled distributor (with built-in coil)
Generator | Alternator (with built-in IC regulator)
Starter motor | Gear reduction drive type

[11B] ENGINE OVERHAUL <4G6-SOHC> - - GENERAL SEPCIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation