[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - INSPECTION CHART FOR TROUBLE SYMPTOMS | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION CHART FOR TROUBLE SYMPTOMS NOTE: If steering movements are made when driving at high speed, or when driving on road surfaces with low frictional resistance, or when passing over bumps, the ABS may operate although sudden braking is not being applied. Because of this, when getting information from the customer, check if the problem occurred while driving under such conditions as these. NOTE: During ABS operation, the brake pedal may vibrate a little or may not be able to be pressed. Such conditions are due to intermittent changes in hydraulic pressure inside the brake line to prevent the wheels from locking. This is normal.
Trouble symptoms | Inspection procedure No. | Reference page
--- | --- | ---
Communication between the MUT-II/III and the whole system is not possible. | - | GROUP 13A, Diagnosis <2000> GROUP 13B, Diagnosis <2400-Except MIVEC> GROUP 13C, Diagnosis <2400-MIVEC>
Communication between the MUT-II/III and the ABS-ECU is not possible. | 1 |
When the ignition key is turned to "ON" (Engine stopped), the ABS warning lamp does not illuminate. | 2 |
The ABS warning lamp remains illuminated after the engine is started. | 3 |
Faulty ABS operation | 4 |

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - INSPECTION CHART FOR TROUBLE SYMPTOMS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation