[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - REFILLING OF OIL IN THE A/C SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

REFILLING OF OIL IN THE A/C SYSTEM Too little oil will provide inadequate compressor lubrication and cause a compressor failure. Too much oil will increase discharge air temperature. When a compressor is installed at the factory, it contains 120 mL <2400-except MIVEC> or 140 mL <2400-MIVEC> of compressor oil. While the A/C system is in operation, the oil is carried through the entire system by the refrigerant. Some of this oil will be trapped and retained in various parts of the system. When the following system components are changed, it is necessary to add oil to the system to replace the oil being removed with the component. Compressor oil: SUN PAG 56 Quantity Evaporator: 60 mL Condenser: 15 mL Flexible suction hose: 10 mL Receiver: 10 mL

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - REFILLING OF OIL IN THE A/C SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation