[42] BODY - - TAILGATE - ON-VEHICLE SERVICE - ADJUSTMENT OF TAILGATE HEIGHT | PRINT PAGE / INDEX / PRIOR / NEXT

| ADJUSTMENT OF TAILGATE HEIGHT
| Turn the tailgate bumper using the arrow of the tailgate bumper as a guideline to adjust the height of the tailgate. The bumper height is altered by approximately 3mm by turning the tailgate bumper one rotation.

[42] BODY - - TAILGATE - ON-VEHICLE SERVICE - ADJUSTMENT OF TAILGATE HEIGHT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation