[42] BODY - - DOOR - DOOR GLASS AND REGULATOR - INSPECTION <EXCEPT VEHICLES FOR HONG KONG SPEC AND ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION <EXCEPT VEHICLES FOR HONG KONG SPEC AND ARGENTINA>
| POWER WINDOW SWITCH CONTINUITY CHECK Remove the power window switch (Refer to GROUP 52A, Door Trim ).
MAIN SWITCH <LH DRIVER VEHICLES>
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
FRONT (LH) | UP | 8 - 13, 9 - 12, | Less than 2 ohms
OFF | 8 - 12, 9 - 12 | Less than 2 ohms
DOWN | 9 - 13, 8 - 12 | Less than 2 ohms
FRONT (RH) | UP | 3 - 13, 11 - 12* | Less than 2 ohms
OFF | 3 - 12*, 11 - 12* | Less than 2 ohms
DOWN | 3 - 12*, 11 - 13 | Less than 2 ohms
REAR (LH) | UP | 1 - 13, 2 - 12* | Less than 2 ohms
OFF | 1 - 12*, 2 - 12* | Less than 2 ohms
DOWN | 1 - 12*, 2 - 13 | Less than 2 ohms
REAR (RH) | UP | 6 - 12*, 13 - 14 | Less than 2 ohms
OFF | 6 - 12*, 12*- 14 | Less than 2 ohms
DOWN | 6 - 13, 12*- 14 | Less than 2 ohms
MAIN SWITCH <RH DRIVER VEHICLES>
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
FRONT (LH) | UP | 3 - 13, 11 - 12 | Less than 2 ohms
OFF | 3 - 12, 11 - 12 | Less than 2 ohms
DOWN | 3 - 12, 11 - 13 | Less than 2 ohms
FRONT (RH) | UP | 8 - 13, 9 - 12* | Less than 2 ohms
OFF | 8 - 12*, 9 - 12* | Less than 2 ohms
DOWN | 9 - 13, 8 - 12* | Less than 2 ohms
REAR (LH) | UP | 1 - 13, 2 - 12* | Less than 2 ohms
OFF | 1 - 12*, 2 - 12* | Less than 2 ohms
DOWN | 1 - 12*, 2 - 13 | Less than 2 ohms
REAR (RH) | UP | 6 - 12*, 13 - 14 | Less than 2 ohms
OFF | 6 - 12*, 12*- 14 | Less than 2 ohms
DOWN | 6 - 13, 12*- 14 | Less than 2 ohms
NOTE: *: Set the window lock switch to UNLOCK position.
SUB SWITCH
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
UP | 5 - 7, 6 - 8 | Less than 2 ohms
OFF | 4 - 7, 6 - 8 | Less than 2 ohms
DOWN | 4 - 7, 5 - 6 | Less than 2 ohms
| POWER WINDOW MOTOR CONTINUITY CHECK
<FRONT DOOR>
TESTER CONNECTION | SLIDER POSITION
--- | ---
Connect terminal No. 4 and the negative battery terminal. Connect terminal No. 1 and the positive battery terminal. | UP
Connect terminal No. 1 and the negative battery terminal. Connect terminal No. 4 and the positive battery terminal. | DOWN
<REAR DOOR>
TESTER CONNECTION | SLIDER POSITION
--- | ---
Connect terminal No. 2 and the negative battery terminal. Connect terminal No. 1 and the positive battery terminal. | UP
Connect terminal No. 1 and the negative battery terminal. Connect terminal No. 2 and the positive battery terminal. | DOWN
| POWER WINDOW MOTOR CHECK Connect a battery directly to the motor terminals and check that the motor runs smoothly. Check that the motor runs in the opposite direction when the battery is connected with the polarity reversed. If defect is found, replace the window regulator as an assembly.

[42] BODY - - DOOR - DOOR GLASS AND REGULATOR - INSPECTION <EXCEPT VEHICLES FOR HONG KONG SPEC AND ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation