[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - GEAR OIL LEVEL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| GEAR OIL LEVEL CHECK Remove the dynamic damper and filler plug.
| Check that gear oil level is not 8 mm below the bottom of filler plug hole. Tighten the filler plug to the specified torque. Tightening torque: 49 ± 9 N·m Tighten the dynamic damper mounting nut to the specified torque. Tightening torque: 44 ± 9 N·m

[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - GEAR OIL LEVEL CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation