[55B] AUTOMATIC AIR CONDITIONER - - EVAPORATOR ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| AIR THERMO SENSOR INSPECTION
| Check to see that the resistance shown in the graph is almost satisfied when measuring the resistance between the terminals under two or more different temperature conditions. NOTE: The temperature should be within the shown range.

[55B] AUTOMATIC AIR CONDITIONER - - EVAPORATOR ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation