[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - Inspection procedure P-21: No photo sensor signal is received. | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection procedure P-21: No photo sensor signal is received.
| CAUTION Whenever the ECU is replaced, ensure that the input signal circuit is normal.
| COMMENTS ON TROUBLE SYMPTOM Input signal from the photo sensor is used to operate the auto lamp function. If the signal is abnormal, the auto lamp function will not work normally.
| POSSIBLE CAUSES Malfunction of photo sensor Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: C-124 photo sensor connector and C-220 ETACS-ECU connector. Q: Is the check result normal? YES: Go to Step 2. NO: Repair the defective connector.
| Step 2. Check the wiring harness from C-124 photo sensor connector terminal Nos. 1, 2, 3 to C-220 ETACS-ECU connector terminal No.27, 28, 26. Check the sensor line for open circuit. Q: Is the check result normal? YES: Go to Step 3. NO: Repair the wiring harness.
| Step 3. ETACS ANALOG data by using the SWS monitor. Vary the illumination intensity of the photo sensor.
Item No. | Item name | Normal condition
--- | --- | ---
Item 01 | PHTO SNR VOLT | The voltage changes within a range of 0.68 to 3.8 V.
OK: Normal condition is displayed. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Go to Step 4.
| Step 4. Replacing the photo sensor Replace the photo sensor (Refer to Group 55 - Photo sensor ). Check that the signals from the photo sensor are received. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - Inspection procedure P-21: No photo sensor signal is received. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation