[23A] AUTOMATIC TRANSMISSION (FF) - - TRANSMISSION CONTROL <L.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

TRANSMISSION CONTROL <L.H. DRIVE VEHICLES>

REMOVAL AND INSTALLATION
WARNING When removing and installing the transmission control cable and shift lock cable unit, be careful not to hit the SRS-ECU.
Pre-removal and Post-installation Operation Front Floor Console Removal. (Refer to GROUP 52A - Floor Console Assembly .)
|  |  | Transmission control cable assembly removal steps
--- | --- | --- | ---
|  | • | Air cleaner assembly (Refer to GROUP 15 - Air cleaner <4G63-SOHC, 4G64>, GROUP 15 - Air cleaner <4G63-DOHC>, GROUP 15 - Air cleaner <4G69>.)
|  | • | Battery and battery tray
| >>B<< | 1. | Transmission control cable assembly connection (transmission side)
| >>A<< | 2. | Shift lock cable unit connection <For Argentina>
|  | 3. | Transmission control cable assembly connection (selector lever assembly side)
|  | 4. | Harness connector
|  | 5. | Selector lever assembly
|  | • | SRS-ECU (Refer to GROUP 52B, SRS control unit .)
|  | 6. | Transmission control cable assembly
|  |  | Selector lever assembly removal steps
| >>A<< | 2. | Shift lock cable unit connection <For Argentina>
|  | 3. | Transmission control cable assembly connection (selector lever assembly side)
|  | 4. | Harness connector
|  | 5. | Selector lever assembly
| INSTALLATION SERVICE POINTS
| >>A<< SHIFT LOCK CABLE UNIT INSTALLATION (For Argentina) Selector lever to P position. Turn the ignition switch to LOCK (OFF) position.
| Install the shift lock cable unit rod to the selector lever assembly lock cam, and tighten the shift lock cable unit installation bolt to the specified torque. Tightening torque: 5.0 ± 1.0 N·m Check the selector lever operation. (Refer to )
| >>B<< TRANSMISSION CONTROL CABLE (TRANSMISSION SIDE) INSTALLATION Place the selector lever and manual control lever in the N position.
| Place the cable stud into the manual control lever slot and install the nut loosely. Gently push the transmission control cable into the manual control lever slot until the cable is taut. Tighten the nut to the specified torque. Tightening torque: 12 ± 2 N·m

[23A] AUTOMATIC TRANSMISSION (FF) - - TRANSMISSION CONTROL <L.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation