[55B] AUTOMATIC AIR CONDITIONER - - AMBIENT TEMPERATURE SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

AMBIENT TEMPERATURE SENSOR

INSPECTION
| Check to see that the resistance shown in the graph is almost satisfied when measuring the resistance between the sensor terminals under two or more different temperature conditions.

[55B] AUTOMATIC AIR CONDITIONER - - AMBIENT TEMPERATURE SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation