[31] WHEEL AND TYRE - - ON-VEHICLE SERVICE - WHEEL RUNOUT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| WHEEL RUNOUT CHECK
| Jack up the vehicle so that the wheels are clear of the floor. While slowly turning the wheel, measure wheel runout with a dial indicator.
Limit:
ITEM | Steel wheel | Aluminium wheel
--- | --- | ---
Radial runout mm | 1.2 | 1.0
Lateral runout mm | 1.2 | 1.0
If wheel runout exceeds the limit, replace the wheel.

[31] WHEEL AND TYRE - - ON-VEHICLE SERVICE - WHEEL RUNOUT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation