[11E] ENGINE MECHANICAL <4G69> - - CRANKSHAFT OIL SEAL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

CRANKSHAFT OIL SEAL

REMOVAL AND INSTALLATION
|  |  | Crankshaft front oil seal removal steps
--- | --- | --- | ---
|  | • | Valve timing belt, balancer timing belt (Refer to ).
| >>D<< | 1. | Crankshaft balancer shaft drive sprocket
|  | 2. | Crankshaft key
| >>C<< | 3. | Crankshaft front oil seal
|  |  | Crankshaft rear oil seal removal steps
|  | • | Transmission assembly (Refer to GROUP 23A, Transmission Assembly ).
<<A>> | >>B<< | 4. | A/T drive plate bolts
|  | 5. | A/T drive plate adapter plate
|  | 6. | A/T drive plate
|  | 7. | Crankshaft bush
| >>A<< | 8. | Crankshaft rear oil seal
| REMOVAL SERVICE POINT
| <<A>> A/T DRIVE PLATE BOLTS REMOVAL
| Use special tool flywheel stopper (MD998781) to secure the A/T drive plate. Remove the A/T drive plate bolts.
| INSTALLATION SERVICE POINTS
| >>A<< CRANKSHAFT REAR OIL SEAL INSTALLATION
| Apply a small amount of engine oil to the entire inner diameter of the oil seal lip. Use the following special tools to press-fit the oil seal. Installer bar (MB990938) Crankshaft rear oil seal installer (MD998776)
| >>B<< A/T DRIVE PLATE BOLTS INSTALLATION
| Use special tool flywheel stopper (MD998781) to secure the A/T drive plate in the same manner as removal. Tighten the A/T drive plate bolts to the specified torque. Tightening torque: 132 ± 5 N·m
| >>C<< CRANKSHAFT FRONT OIL SEAL INSTALLATION
| Apply a small amount of engine oil to the outer diameter of special tool crankshaft front oil seal guide (MD998285) and install it to the crankshaft. Apply a small amount of engine oil to the entire inner diameter of the oil seal lip. Use special tool crankshaft front oil seal installer (MD998375) to press-fit the oil seal.
| >>D<< CRANKSHAFT BALANCER SHAFT DRIVE SPROCKET INSTALLATION
| Clean or degrease the front case, the crankshaft and the crankshaft balancer shaft drive sprocket as shown. NOTE: Also clean the degreased surfaces. Install the crankshaft balancer shaft drive sprocket in the direction shown in the illustration.

[11E] ENGINE MECHANICAL <4G69> - - CRANKSHAFT OIL SEAL - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation