[35A] BASIC BRAKE SYSTEM - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value | Limit
--- | --- | ---
Brake pedal height mm | LH drive vehicles | 150 - 153 | -
RH drive vehicles | 176.2 - 179.2 | -
Brake pedal free play mm | 3 - 8 | -
Brake pedal to floor board clearance mm | 100 or more | -
Proportioning valve output fluid pressure MPa <Vehicles without ABS> | Split point | 3.19 - 3.67 | -
When input fluid pressure is 7.35 MPa. | 4.17 - 4.66 | -
Proportioning valve output fluid pressure difference between left and right MPa | - | 0.5
Disc brake pad thickness mm | 10.0 | 2.0
Disc brake disc thickness mm | Front (1-piston type) | 26.0 | 24.4
Front (2-piston type) | 24.0 | 22.4
Rear | 10.0 | 8.4
Disc brake disc run-out mm | Front | - | 0.04
Rear | - | 0.05
Front disc brake drags force N | Front (Except for 2000-DOHC) | 68 or less | -
Front (Vehicle for 2000-DOHC) | 77 or less | -
Rear | 68 or less | -
Rear drum brake lining thickness mm | 4.9 | 1.0
Rear drum inside diameter mm | 228.6 | 230.6
Front hub axial play mm | - | 0.05
Brake booster push rod protruding length mm (When applying negative pressure of 66.7 kPa to the brake booster) | 10.15 - 10.40 | -

[35A] BASIC BRAKE SYSTEM - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation